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TERRACE ventilated 

	☐ TILES 
	☐ DECKING

	Basic information

	Investor
	

	Address realization
	

	Floor
	

	Elevator
	YES
	NO
	Consider that no elevator and the need to bring the material may be an additional expense

	Bringing
	YES
	NO
	

	Artist terrace
	Editing self
	Outsourcing company
	

	details contact the company that installed the terrace
	


	Expected date execution of the installation
	



	Detailed information about the terrace

	Purpose of the terrace
	Recreational / public / fountain / restaurant / SPA (jacuzzi) / internal / technical
other
	

	Area m2
	
	

	Fixed 0 point of the terrace
	Lower window frame / floor level inside
other

	Most often the zero point of the terrace is the bottom window frame or the level floors inside the room adjacent to the terrace. 

	Substrate type under pedestals
	Styrodur XPS, heat-sealable roofing felt, liquid waterproofing, concrete, tiles, cubes, concrete blocks,native soil
	Styrodur XPS300 is the recommended hardness for positioning the pedestals.

	Stability and evenness of the substrate
	
	The substrate should provide stable support for the pedestals to avoid excessive bending of the terrace during use.

	Damage-Damage-
	
	sensitive substrate sensitive substrate, such as liquid waterproofing, should be additionally secured with a SBR 200x200 rubber pad under the bracket.

	Possibility of anchoring the pedestals to the ground
	YES
	NO
	The pedestals cannot be anchored on the ground with waterproofing functions.

	Declines on the terrace
	
	

	Minimum height 
	
	The lowest adjustable support DD PEDESTALS has a height of 10 mm.

	Maximum height The
	
	highest adjustable bracket DD PEDESTALS is 950 mm high.

	Laying the terrace
	horizontally
	In a slope
	A terrace made of plates arranged horizontally or with a minimum slope of 0.5-1.0% looks the best.

	Finishing of the terrace from the outside
	
	If the terrace has exposed edges, it is necessary to provide for the installation of the masking frames.



	Information for terrace BOARDS

	size plate
	
	

	thickness of the plate
	
	

	Manufacturer plate
	
	

	Model / name plate
	
	

	Is the disc keeps the same thickness
	YES
	NO

	If you select NI is recommended to use rubber pads SH to bridge the gap plates

	Manufacturer's recommendation for board support pedestals
	only in the corners / In the corners and in the middle / other …………………… ..
	Each panel manufacturer should provide information whether they allow point support of the panels and on what conditions

	The gap between the panels
	3 mm / 5 mm
	3 mm recommended for panels with an even edge, 5 mm recommended for boards with slight edge line deviations (then it is less visible). Water will flow freely from the terrace already at a width of 3 mm.



	Information for the PLANK TERRACE

	Plank type
	Wood, WPC composite 
other
	

	Plank profile Plank
	
	

	type
	stoneware, concrete, stone
other 
	

	Board manufacturer's recommendations regarding the distance between the
	
	

	Joist type
	Wood, composite, aluminum
Other

	

	Joist profile Joist
	
	

	Joists manufacturer's recommendations regarding the distance between supports on the supports
	
	



	To The list should be attached with a drawing of the terrace

	Checklist what should be included in the drawing:
☐ All terrace dimensions have been marked
☐ The terrace has edges shown.
☐ The lowest and highest point of the terrace
☐ Slopes on the terrace have been drawn
☐ Water drains have been marked 
☐ Stairs and changes in the height of the terrace surface have been marked 
☐ The necessary revisions
☐ Needed point where extra support is needed (eg. jacuzzi bath etc.) 
☐ Installations under the terrace (electric, hydraulic pipes etc.)
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